上海山美重型矿山机械有限公司是中国领先的破碎筛分设备制造商，是德国哈兹马克公司在中国的合资公司。我们能够给客户提供全系列破碎筛分设备和完整解决方案，产品包括圆锥破碎机、颚式破碎机、反击式破碎机、立式冲击破碎机（制砂机）、振动筛、细砂回收系统、轮式移动破碎站和履带式移动破碎站。我们的目标是为全球客户提供值得信赖的产品和服务，为客户创造价值。

Shanghai Sanme Mining Machinery Co.,Ltd is a leading manufacturer of crushing and screening equipments in China, a joint venture with HAZEMAG Germany. We can offer full range of crushing and screening equipment, including cone crusher, jaw crusher, impacter, VSI (Sand Maker), screen, fine sand collecting system, portable crushing plant and mobile crushing plants, but also provide total solutions. Our aim is to provide reliable products and services for global customers and create values for our customers.

**欧星MP-C系列履带移动圆锥式破碎站**

**MP-C Series Mobile Cone Crushing Plants**

欧星MP-C系列履带移动圆锥式破碎站采用德国技术设计和制造，达到了国际先进水平，在设计中广泛采用了世界上最先进的移动破碎技术，能够完全满足客户的移动破碎要求，改变您的盈利模式。

Designed and manufactured with German technology, MP-C Series Mobile Cone Crushing Plants have reached the world advanced level. The plant adopts first level mobile crushing technique, which fully meets the customers' requirement of high mobility, high crushing efficiency and optimizes your business mode.

**欧星MP-C系列履带移动圆锥式破碎站可以应用于：**

**MP-C Series Mobile Cone Crushing Plants are applicable for:**

◆ 矿物和硬岩破碎

◆ 砂石骨料生产

◆ 钢渣处理

◆ 隧道破碎

◆ Minerals and Hard rock Crushing

◆ Aggregates Processing

◆ Slag Processing

◆ Tunnel Crushing



**技术参数：**

**Technical Specifications:**

|  |  |  |  |
| --- | --- | --- | --- |
| **MP-C系列履带移动圆锥式破碎站****MP-C Series Mobile Cone Crusher Plants** | **MP-C120** | **MP-C180** | **MP-C250** |
| **圆锥破碎机型号 Cone Crusher** | **SMH120** | **SMH180** | **SMH250** |
| **最大进料粒度 Max Feed Size(mm)** | 160 | 180 | 260 |
| **排矿口调整范围 Gap Width(mm)** | 9-32 | 9-32 | 9-51 |
| **处理量 Crushing Capacity(t/h)** | 最大 up to 150 | 最大 up to 200 | 最大 up to 350 |
| **动力装置 Driving Unit** |
| **发动机 Engine** | Cummins or CAT | Cummins or CAT | Cummins or CAT |
| **功率 Performance（kw）** | 261 | 261 | 400 |
| **给料斗 Feed Hopper** |
| **料斗容积 Hopper Volume（m3）** | 4 | 5 | 6 |
| **带式给料机 Belt Feeder** |
| **驱动方式 Drive** | 液压 hydraulic | 液压 hydraulic | 液压 hydraulic |
| **主皮带机 Main Conveyor belt** |
| **卸料高度 Discharge Height（mm）** | 2900 | 3300 | 3300 |
| **驱动方式 Drive** | 液压 hydraulic | 液压 hydraulic | 液压 hydraulic |
| **履带行走装置 Crawler Unit** |
| **驱动方式 Drive** | 液压 hydraulic | 液压 hydraulic | 液压 hydraulic |
| **外形尺寸和重量 Dimensions and Weight** |
| **工作状态外形尺寸 Working Dimensions** |
| **-长度 Length(mm)** | 13767 | 13850 | 14530 |
| **-宽度 Width(mm)** | 3621 | 3650 | 4150 |
| **-高度 Height(mm)** | 4497 | 4550 | 4720 |
| **运输状态外形尺寸 Transport Dimensions** |
| **- 长度 Length(mm)** | 14273 | 14320 | 14900 |
| **- 宽度 Width(mm)** | 3543 | 3570 | 3640 |
| **- 高度 Height(mm)** | 4024 | 4050 | 4130 |
| **重量 Weight(t)** | 37 | 39.5 | 49 |

注：上述生产能力是在破碎物料堆比重为1.6t/m3时开路循环生产中总吨数。生产能力与破碎物料的物理性能、给料方式、进料粒度及其组成等工况有关。

Note: Capacity is total tons per hour passing through crusher at open circuit when bulk density of feeding is 1.6t/m³. Capacities are relative to physics character and type of feeding, feeding size and composition.