****

**RCYB系列悬挂式永磁除铁器**

**RCYB Series of Manual-Cleaning Permanent Magnetic Separator**



**适用范围：**

适用于皮带输送机、振动给料机、下料溜槽上的非磁性物料中除铁。

**Applicable scope:**

removal of iron in non-magnetic materials on belt conveyor, vibrating feeder and blanking chute.

**技术参数** **Technical Data:**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **型号****Model** | **适应宽度****Belt width Adaptive(mm)** | **悬挂高度****Suspension Height Rated(mm)** | **适应带速****Belt Velocity(m/s)** | **物料厚度****Material Thickness (mm)** | **重量****Weight(kg)** | **外型尺寸****Overall Dimensions(L×W×H)mm** |
| RCYB-5 | 500 | 150 | 4.5 | 900 | 206 | 500 | 350 | 260 |
| RCYB-6.5 | 650 | 200 | 4.5 | 150 | 450 | 650 | 600 | 300 |
| RCYB-8 | 800 | 250 | 4.5 | 200 | 680 | 950 | 950 | 380 |
| RCYB-10 | 1000 | 300 | 4.5 | 250 | 1180 | 1100 | 1000 | 380 |
| RCYB-12 | 1200 | 350 | 4.5 | 300 | 1670 | 1300 | 1340 | 420 |
| RCYB-14 | 1400 | 400 | 4.5 | 350 | 2350 | 1500 | 1500 | 420 |

**RCYD系列永磁自卸式除铁器**

**RCYD Series Belt Permanent Magnetic Separator**

****

**适用范围：**

本机与各种皮带输送机、振动给料机等配套使用，可用于从运动的物料中自动吸除0.1-35kg的铁磁性物质。广泛应用于水泥、冶金、矿山、玻璃、煤炭等行业。

**Applicable scope:**

It is used together with belt conveyor, vibrating feeder, etc; applicable to automatic removal of 0.1-35kg ferro-magnetic materials from moving materials, and extensively applied in cement, metallurgy, mine, glass, coal and other industries.



**技术参数** **Technical Data:**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **型号****Model** | **适用带宽****Belt width Adaptive****(mm)** | **额定吊高****Suspension Height Rated****(mm)** | **磁场强度****Magnetic Intensity SHR(mT)** | **物料厚度****Material Thickness (mm)** | **电机功率****Motor Power****(mw)** | **适应带速****Belt Velocity(m/s)** | **重量****Weight****(kg)** | **外型尺寸****Overall Dimensions****(L×W×H)mm** |
| RCYD-5 | 500 | 150 | 60 | 80 | 1.5 | 4.5 | 750 | 1900 | 735 | 935 |
| RCYD-6.5 | 650 | 200 | 70 | 150 | 2.2 | 4.5 | 1200 | 2165 | 780 | 1080 |
| RCYD-8 | 800 | 250 | 70 | 200 | 2.2 | 4.5 | 1400 | 2350 | 796 | 1280 |
| RCYD-10 | 1000 | 300 | 70 | 250 | 3.0 | 4.5 | 2120 | 2660 | 920 | 1550 |
| RCYD-12 | 1200 | 350 | 70 | 300 | 4.0 | 4.5 | 3350 | 2900 | 970 | 1720 |
| RCYD-14 | 1400 | 400 | 70 | 350 | 4.0 | 4.5 | 4450 | 3225 | 1050 | 1980 |