**XL系列洗砂机**

**XL Series Sand Washer**





XL系列洗砂机可清洗分离砂石中的泥土和杂物，其新颖的密封结构、可调溢流堰板、可靠的传动装置确保清洗脱水的效果，适用于公路、水电、建筑等行业。

XL Series Sand Washer can wash and separate the soil and foreign material in the sand. Its novel structure, adjustable overflow dam baffle and reliable arrangement can make sure the result of wash.

**技术参数** **Technical Data:**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **型号****Model** | XL508 | XL610 | XL762 | XL915 | 2XL915 | XL1115 | 2XL1115 |
| **螺旋直径****Screw Diameter(mm)** | 508 | 610 | 762 | 915 | 915 | 1115 | 1115 |
| **槽体长度****Length of Tub(mm)** | 6705 | 7225 | 7620 | 7585 | 7585 | 9782 | 9782 |
| **最大入料粒度****Max Feed Size(mm)** | ≤10 | ≤10 | ≤10 | ≤10 | ≤10 | ≤10 | ≤10 |
| **生产能力****Capacity(t/h)** | 20 | 40-50 | 50-75 | 100 | 200 | 175 | 350 |
| **螺旋转速****Speed of Screw(r/min)** | 38 | 32 | 26 | 21 | 21 | 17 | 17 |
| **电机功率****Motor Power(kw)** | 5.5 | 7.5 | 11 | 11 | 2×11 | 15 | 2×15 |
| **耗水量****Water Consumption(t/h)** | 6-60 | 6-63 | 9-63 | 10-80 | 20-160 | 20-150 | 40-300 |
| **外型尺寸****Overall Dimensions(L×W×H)(mm)** | 8000×2343×1430 | 8000×2050×1400 | 8545×2650×3862 | 8500×2810×3600 | 8420×3765×3960 | 10970×3945×4720 | 10970×5250×4720 |
| **重量****Weight(t)** | 2.67 | 3.80 | 5.23 | 6.27 | 11.11 | 10.18 | 17.94 |